Underwater Investigations and Robotics. 2020. No. 1 (31). P. 21–30.

About the accuracy of positioning the underwater module based on measured movement parameters of a towed system

**Dubrovin F.S., Vaulin Yu.V., Kostenko V.V., Lvov O.Yu.**

Institute for Marine Technology Problems FEB RAS

5a, Sukhanov Str., Vladivostok, 690950. Ph.: +7 (423) 243-24-16.
E-mail: kostenko@marine.febras.ru

**ABSTRACT**

The towed underwater module (TUM) is a useful tool for solving problems of the positioning of the underwater objects, the location of which must be clarified during its detailed inspection. Herewith, the accuracy of the determination of the coordinates of the towed module itself relative to the towing vessel is essential for such kind of problems. The use of underwater acoustic navigation means, the systems with ultra-short baseline (USBL) in particular, are limited due to interference affecting the quality of the signals on the receiving antenna. As an alternative, the method is proposed for TUM positioning based on trajectory measurements of parameters of the towed system, which may include calculated values of communication cable parameters in steady-state towing modes, values of ground speed and towing angle, as well as measured cable length, immersion depth, and TUM heading. The paper provides a comparative analysis of various versions of computational algorithms, which allow obtaining estimates of the TUM positioning accuracy in different modes of stationary towing and in the presence of failures in navigation systems operation.

**Key words:** towed underwater module, sonar navigation system, load-bearing communication cable, satellite navigation receiver, coordinate determination algorithms.

**REFERENCES**

1. Rimskiy-Korsakov N.A. *Tekhnicheskie sredstva dlya issledovaniya dna akvatoriy gidrolokatsionnymi metodami // Mezhdunarodnyy zhurnal prikladnykh i fundamental'nykh issledovaniy.* 2017. No. 10–2. P. 205–213. – URL: https://www.applied-research.ru/ru/article/view?id=11889 (usage date: 11.02.2020).
2. Miln P.Kh. *Gidroakusticheskie sistemy pozitsionirovaniya: per. s angl.* L.: Sudostroenie, 1981. 304 p.
3. Thomas H.G. GIB buoys: an interface between space and depths of the oceans // Proc. of the 1998 Workshop on Autonomous Underwater Vehicles (Cat. No.98CH36290). Cambridge, MA, USA, 1998. P. 181–184. doi: 10.1109/AUV.1998.744453.
4. Boreyko A.A., Vaulin Yu.V., Dubrovin F.S., Shcherbatyuk A.F. *Sovremennye podkhody k organizatsii navigatsionnogo obespecheniya raboty morskikh robototekhnicheskikh kompleksov IPMT DVO RAN: Dokl. na XIII Vseros. soveshch. po problemam upravleniya* (VSPU-2019)). – URL: https://vspu2019.ipu.ru/files/vspu/Doklady%20VSPU2019/18\_V\_A7/BoreykoAA.pdf (usage date: 12.02.2020).
5. *Podvodnye robototekhnicheskie kompleksy: sistemy, tekhnologii, primenenie* /A.V. Inzartsev, L.V. Kiselev, V.V. Kostenko, Yu.V. Matvienko, A.M. Pavin, A.F. Shcherbatyuk; [otv. red. L.V. Kiselev]; FGBUN In-t problem morskikh tekhnologiy DVO RAN. Vladivostok, 2018. 368 s. ISBN 978-5-7311-0486-79.
6. Kebkal K.G., Kebkal O.G., Bannasch R., Yakovlev S. Performance of a Combined USBL Positioning and Communication System Using S2C Technology // Proc. of the Int. Conf. OCEANS-2012. Yeosu. 2012. P. 1–7.
7. Borodin V.I. et al. *Gidroakusticheskie navigatsionnye sredstva.* L: Sudostroenie, 1983. 262 s.
8. Herman D.A., Kostenko V.V., Mokeeva I.G. Choice of ROV’s thruster set power according to footprint’s radius on steady motion // Proc. of the OCEANS 94 «Oceans Engineering for Today’s Technology and Tomorrow’s Preservation». Choice of ROV’s thruster set power according to footprint’s radius on steady motion. Brest, 1994. Vol. 3. P. 453–456. doi: 10.1109/OCEANS.1994.364241.
9. Kostenko V.V., Mokeeva I.G. *Issledovanie vliyaniya kabelya svyazi na manevrennost' teleupravlyaemogo podvodnogo apparata* [Research of tie cable influence on ROV's maneuverability] // *Podvodnye issledovaniya i robototekhnika* [Underwater Investigations and Robotics]. 2009. No. 1 (7). C. 22–27.
10. Vaulin Yu.V., Kostenko V.V., Mokeeva I.G., Matvienko Yu.V., Rylov N.I. *Osobennosti koordinirovaniya donnykh istochnikov navigatsionnykh signalov s ispol'zovaniem buksiruemogo antennogo modulya* [Traits of bottom sonar sources of navigation signal coordination with use of towed antenna module] // Podvodnye issledovaniya i robototekhnika [Underwater Investigations and Robotics]. 2018. No. 2 (26). P. 4–11.
11. Kostenko V.V., L'vov O.Yu. *Kombinirovannaya sistema svyazi i navigatsii avtonomnogo podvodnogo robota s poplavkovym modulem* [Combined systems of communication and navigation for autonomous underwater robot equipped with a float towed unit] // *Podvodnye issledovaniya i robototekhnika* [Underwater Investigations and Robotics]. 2017. No. 1 (23). P. 31–43.
12. Crawford А.М. 2002. Methods for Determining Towfish Location for Improvement of Sidescan Sonar Image Positioning. DREA TM 2002-019. Defence R&D Canada – Atlantic.  – URL: https://pdfs.semanticscholar.org/f60c/529d949ff1e0aefcb84ca22b975bdcedf298.pdf (usage date: 12.02.2020).
13. EvoLogics S2C R 15/27 USBL communication and positioning device. – URL: https://evologics.de/acoustic-modem/15-27/usbl-serie (usage date: 12.02.2020).
14. Applanix POS MV V5 – Position and Orientation System for Marine Vessels. – URL: https://seatronics-group.com/files/9614/1753/5309/Applanix\_POS\_MV-Manual.pdf (дата обра-щения: 12.02.2020).GPS/GLONASS/SBAS Receiver NV08C-RTK GNSS Card
15. Datasheet. – URL: https://www.diltronic.com/wp-content/uploads/2015/01/NV08C-RTK-DS-v1-0-ENG-30-12-2014.pdf (usage date: 12.02.2020).